EM425 Assignment #9

Problem Statements

1. (Based on 11.14) Write a user-defined MATLAB function that solves, with the shooting method in conjunction with the secant method, a second-order boundary value problem of the form:



Where  and  are constants. For the function name and arguments use [x,y]=BVPShootSecant(Fx,Gx,Hx,a,b,n,Ya,Yb,Wa,Wb). The input arguments Fx, Gx, and Hx are names for the functions that calculate  respectively. The arguments a and b define the domain of the solution, n is the number of subintervals, Ya and Yb are the boundary conditions, and Wa and Wb are the assumed slopes at  that are used in the first two iterations of the Secant Method. Within the user-defined function BVPShootSecant, use the function odesCRK4 that you created in Assignment #8. The secant method should be carried out until the absolute value of the true error at  is smaller than 0.001.


Use this function to solve the following boundary value problem:



With boundary conditions: .

Use  and 

Plot the solution.

2. (Based on 11.21) A cylindrical pipe with inner radius 1 cm and wall thickness 2.5 cm carries a fluid at a temperature of 600oC. The outer wall of the pipe is at 25oC. The governing equation for the temperature distribution in the pipe wall is:



Subject to the boundary conditions T(1) = 600oC and T(3.5) = 25oC. Solve for the temperature  and plot the temperature distribution.

Part a)

1. Solve using BVPShootSecant that you created for problem #1
2. Solve using bvp5c.

Plot the solution using both methods and output the value of  using both methods.

Part b)

What is the physical significance of the right-hand side (-500) in the governing equation? (i.e. what conservation law is being expressed with the governing equation?) What happens to the temperature profile when the right-hand side is made much bigger?

Part c)

Replace the boundary condition at r = 3.5 to model convective heat transfer to a fluid medium maintained at 25oC. Assume a convective heat transfer coefficient of 1.5 W/cm2-K.



Solve the problem using bvp5c, plot the temperature profile and output the T(r = 3.5). Experiment with different values of convective heat transfer coefficient to make sure the response is as you expect. What happens as the convective heat transfer coefficient gets very large? What happens when it gets small? Briefly describe your observation. (no more than a paragraph with supporting plots)

3. (Based on 11.27) The radial distribution of temperature in a current-carrying bare wire is described by:



Where  is the temperature in K,  is the radial coordinate in m,  is the thermal conductivity,  is the current,  is the electrical resistivity, and  m is the wire diameter. Use MATLAB’s built-in function bvp5c to solve the equation for . Solve twice for the following boundary conditions:

1. At  m,  and at  
2. At  and at  where  W/m2-K is the convective heat transfer coefficient and  = 300K is the ambient temperature.

Important note:  is a singular point and must therefore be replaced with a small, non-zero value -- e.g. 10-6. As initial guesses, use T = 500K and  use 50 subintervals.

For both parts a) and b), plot the temperature profiles and output the difference in temperature between the centerline of the wire and the outer surface of the wire. Give a brief physical explanation for the differences in the temperature profiles for part a and b. (no more than a couple of sentences)

**Solutions:**

